# Menu 1 − Regen References

Mode: Regeneration

Parameter | 01.054 Fire Mode Activate
--- | ---
Short description | Set to 1 to activate fire mode
Mode | Regeneration
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit Volatile | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RO, NC

Fire Mode Activate (01.054) cannot be written directly, but it can be controlled from a digital input. This prevents fire mode from being enabled from the keypad, comms or an option module.

Fire mode is intended for purging air from a ventilation system in the event of a fire. All trips are either disabled or are automatically reset after 1s. The use of fire mode can result in damage to the drive, and so if fire mode is enabled and any trip is initiated an indication that cannot be reset by the user is stored in Potential Drive Damage Conditions (10.106). For Open-loop, RFC-A or RFC-S modes fire mode is activated and if Fire Mode Reference (01.053) has a non-zero value and Fire Mode Activate (01.054) = 1. When fire mode is activated normal drive operation is overridden as follows.

1. Pre-ramp Reference (01.003) is forced to the value in Fire Mode Reference (01.053).
2. The Final drive enable is forced to be active provided the safe torque off hardware input will allow the drive to be enabled. The Final drive run is forced to be active.
3. Forward Limit Switch (06.035) and Reverse Limit Switch (06.036) are disabled.
4. Hard Speed Reference (03.022) is forced to 0 (RFC-A and RFC-S modes). The hard speed reference should not be used when fire mode can be activated as this could cause an abrupt change in speed.
5. The hand/off/auto system is disabled. If this system is in the hand state when fire mode is activated it will be forced to the off state, so that hand state is not active when fire mode is de-activated.
6. Keypad control mode is disabled.
7. All latched states in the sequencer (Menu 6) are reset.

For Regen mode fire mode is activated if Fire Mode Activate (01.054) = 1. When fire mode is activated the Final drive enable is forced to be active provided the safe torque off hardware input will allow the drive to be enabled.

If the drive is in the tripped state when fire mode is activated the trip is reset and then only the trips listed in the table below can be initiated whilst fire mode is active. If any of the trips shown as resettable occur, the drive will attempt to automatically reset the trip after 1s.

Trip number | Trip | Resettable
2 | Over Volts | Yes
3 | OI ac | Yes
4 | OI Brake | Yes
5 | PSU | Yes
9 | PSU 24V | Yes
21 | OHt Inverter | Yes
31 | EEPROM Fail | No
36 | User Save | No
37 | Power Down Save | No
109 | OI dc | Yes
200 | Slot1 HF | No
205 | Slot2 HF | No
210 | Slot3 HF | No
217-249 |  | No
250 | Slot4 HF | No